**Liquid Tight Conduit**



Liquid Tight Conduit

* Use a liquid tight ﬂexible conduit a conductors with a nominal rating of
* Sizes 3/8" to 2"
* Integral rigid and ﬂexible PVC cons
* Dry temp. rating: 0º to 176º F (-18
* In Oil temp. rating: up to 160º F (70
* Wet temp. rating: up to 140º F (60º
* Use straight-thru and right-angle c